# HANGING PLOT – The Wedge Performing Arts Centre



SHOW-:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

|  |  |  |  |  |  |
| --- | --- | --- | --- | --- | --- |
| *Line Number* | *Distance from Setting Line* | *Drive Mechanism*  *Chain Motor / Hand Winch* | *Standard Position* | *Required Position* | *Notes* |
| 1 | 200 mm | Hand Winch | Frieze | Frieze | Not an actual bar. |
| 2 | 300 mm | Dead Hung | House Curtain | House Curtain | Fixed. |
| 3 |  |  |  |  |  |
| 4 | 700 mm | Hand Winch | Border 1 |  |  |
| 5 | 1000 mm | Chain Motor | LX 1 |  |  |
| 6 | n/a | n/a | n/a | n/a | n/a |
| 7 | 1500 mm | Hand Winch | Legs 1 |  |  |
| 8 | 1800 mm | Chain Motor |  |  |  |
| 9 | n/a | n/a | Projection Screen | n/a | Not an actual bar. |
| 10 | 2400 mm | Hand Winch | Border 2 |  |  |
| 11 | 2700 mm | Chain Motor | LX 2 |  |  |
| 12 | 3000 mm | Hand Winch | Legs 2 |  |  |
| 13 | 3300 mm | Chain Motor | Black wool Tabs |  |  |
| 14 | 3650 mm | Hand Winch |  |  |  |
| 15 | n/a | n/a | n/a | n/a | n/a |
| 16 | 4300 mm | Chain Motor | Legs 3 |  |  |
| 17 | 4500 mm | Hand Winch | Border 3 |  |  |
| 18 | n/a | n/a | n/a | n/a | n/a |
| 19 | 5100 mm | Chain Motor | LX 3 |  |  |
| 20 | 5400 mm | Chain Motor |  |  |  |
| 21 | 5700 mm | Chain Motor | Legs 4 |  |  |
| 22 | 6050 mm | Hand Winch | Border 4 |  |  |
| 23 | 6300 mm | Chain Motor | LX4 |  |  |
| 24 | 6600 mm | Hand Winch |  |  |  |
| 25 | n/a | n/a | n/a | n/a | n/a |
| 26 | 7100 mm | Chain Motor |  |  |  |
| 27 | 7400 mm | Chain Motor | Black wool Tabs |  |  |
| 28 | 7650 mm | Hand Winch | Cyclorama |  |  |

Please Note: Venue Preference is Heavier Bars such as LX etc are preferred to be on Chain Motor Operated lines.